1. RFC 1350
   1. Overview of the protocol
      1. Any transfer begins with a request to read or write a file. This also serves as a request to connection.
      2. When granted by the server, the connection is opened with the file being sent in a fixed length blocks of 512 bytes.
      3. Each data packet contains one block of data and must be acknowledged by an acknowledgement packet before the next packet can be sent.
      4. Any data packet sent with less than 512 bytes signals the termination of a transfer.
2. RFC 2347
3. RFC 2348
4. RFC 2349